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	PROCEDURE
	WEEKLY
	MONTHLY
	YEARLY

	1. Check system operating pressures and temperatures.
	x
	 
	 

	2. Check oil level.
	x
	 
	 

	3. Check condition of oil.
	
	x 
	 

	4. Check liquid injection operation.
	 
	x
	 

	5. Check operation of capacity control device (slider & solenoid valves)
	 
	x
	 

	6. Check crankcase heater operation.
	 
	x
	 

	7. Sample compressor oil.
	 
	 
	x

	8. Check integral check valve
	 
	 
	x 

	9. Check pressure relief valve and roller bearings
	 
	 
	x

	10. Check for pipework damages Near to Chiller.
	 
	x
	 

	11. Check filter drier
	 
	x
	 

	12. Check for leaks (complete leak check)
	 
	 
	 x

	13. Check liquid line sight glass / moisture indicator
	x
	 
	 

	14. Check suction superheat at compressor
	x
	 
	 

	15. Check condenser liquid subcooling
	x
	 
	 

	16. Check expansion valves, solenoid valves and check valves.
	 
	x
	 

	17. Check condenser coils for dirt / debris and clean as required.
	 
	x
	 

	18 Check fans and fan guards.
	 
	x
	 

	19. Check fan motor bearings.
	 
	 
	 x 

	20. Check water flow.
	 
	x
	 

	21. Check water pressure drop & cooler efficiency.
	 
	x
	 

	22. Check cooler heater operation (if provided).
	 
	x
	 

	23. Check water pH / glycol strength.
	 
	 
	x

	24. Check condition of control panel and all components
	 
	x
	 

	25. Check power and control wiring.
	 
	x
	 

	26. Check sensor locations.
	 
	x
	 

	27. Check mechanical HP cut-outs and water flow switch operation.
	 
	x
	 

	28. Check under voltage monitor and main disconnect.
	 
	x
	 

	29. Check tightness of all wiring connections
	 
	 
	x

	30. Check compressor contactors/ overloads/ breakers.
	 
	 
	x

	31. Check fan contactors / breakers.
	 
	 
	x

	32. Check sensor / transducer calibration
	 
	 
	x

	33. Check compressor motor protectors.
	 
	 
	x

	34. Check contactor contacts.
	 
	 
	x

	35. Check fault history
	x
	 
	 

	36. Check operating set points.
	 
	x
	 

	37. Check HP and OP safety cut-out function.
	 
	x
	 

	38. Check pump-down function.
	 
	 
	 x 

	39. Check capacity load / unload function.
	 
	 
	 x 

	40. Check fan control function.
	 
	 
	  x

	41. Check ambient cut-out function.
	 
	 
	  x

	42. Check thermal insulation on cooler and piping.
	 
	x
	 

	43. Check vibration isolators, repair/replace as necessary
	 
	x
	 

	44. Check unit structure for loose bolts/ screws and tight as necessary
	 
	 
	x

	45. Check for rusted/dented/ damaged body parts and repair/ repaint as necessary.
	 
	 
	x




